**PIEZOELECTRIC BUZZER**

**MICRO BUZZER 5V DC / 20mA PCB TYPE**



**Features**

* + sealed: yes
  + operating power: 3-6V DC / 25mA
  + extremely compact, ultrathin construction
  + no electrical noise
  + low current consumption yet high sound pressure level

**Specifications**

* tone type: single
* operating voltage: 3-6V DC
* rated voltage: 5V DC
* current consumption: 25mA
* osc. frequency: 3.2kHz
* sound level: 87dB
* connector type: pcb
* body color: gray
* weight: 0.056oz